AT-ETX-2I

Bill of Materials

1. RAD products:

|  |  |  |
| --- | --- | --- |
|  | For 4 units |  |
| ACE-3200/AC/S2/8E1 | 1 |  |
| RM-34 (for ATE-PIO-USB, ATE-MMUX) | 11 |  |
| RM-35/P2 (for ETX204 ) | 2 |  |
| ETX-204A/AC/4 with Ethernet Generator program | 4 |  |
| RINGER-2200N | 8 |  |
| RING-2200-RM | 8 |  |

1. A.T.E. products:

|  |  |  |
| --- | --- | --- |
|  | For 4 units |  |
| ATE-PIO-USB | 4 |  |
| ATE-RELAY-BOX-4 | 2 |  |
| ATE-MultiMux | 4 |  |

1. Cables:
   1. RAD cables:

|  |  |  |
| --- | --- | --- |
|  | For 4 units |  |
| CBL-DB9F-DB9M-STR | 6 |  |
| CBL-ETH/STP/STR | 13 |  |
| CBL-MUSB-DB9F | 4 |  |

* 1. Specify cables:

|  |  |  |
| --- | --- | --- |
|  | For 4 units |  |
| AT-ETX2i/CBL01 | 1 |  |
| AT-ETX2i/CBL02 | 1 |  |
| AT-ETX2i/CBL03 | 2 |  |
| AT-ETX2i/CBL04 | 8 |  |
| AT-ETX2i/CBL05 | 4 |  |
| AT-ETX2i/CBL06 | 4 |  |

1. Mechanic parts:

|  |  |  |
| --- | --- | --- |
|  | For 4 units |  |
| Masad (width 19”) | 1 (height 32U) |  |
| Fixed Shelf | 1 |  |
| Removeable Shelf | 4 |  |

1. Test equipment
   1. PC’s card

|  |  |  |
| --- | --- | --- |
|  | For 4 units |  |
| Ethernet card | 2 |  |

* 1. Movable equipment

|  |  |  |
| --- | --- | --- |
|  | For 4 units |  |
| Barcode scanner | 1 |  |
| USB-4xRS232 | 2 |  |
| 8 port 10/100 Ethernet Switch | 1 |  |

1. PC
   1. PC
   2. Screen
   3. Keyboard
   4. Mouse
2. Miscellaneous:
   1. 5-way long power cable 230v …...…..…… 2 units
   2. Extension power cable 230v ..………..…… 1 unit
   3. Multiple power socket ..…………………… 1 unit
   4. Mouse pad …………………………....…… 1 unit
   5. Anti static surface ……………………….…. 4 units